{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":4},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":6,"rows_kept":9,"merged":[[0,0,0,5]]}
["道闸系统设备参数表"]
["序号","名称","主要参数及要求","数量","单位","参考外观"]
[1,"分体式车牌识别","摄像头：500万高清摄像头支持直连云，0.1秒快速识别，支持智能化视频检测抓拍，实现机动车精准抓拍识别，识别率大于等于99.7%；\n显示屏 ：21.5寸LCD液晶屏\n外观尺寸：380*210*1500mm\n相机镜头：2.8-12mm变焦镜头，专有低照度技术保障成像效果，夜间看的更清；\n集成度高：集摄像机、LED显示屏（可选）、LED补光灯、镜头、喇叭功放于一体，有效节省施工布线成本；\n智能补光技术：支持时控和光控，满足不同场景需求\n车牌识别种类：支持识别的号牌类型包括大（小）型汽车、新能源汽车\n授权名单控制：支持授权名单的导入及对比，可直接联动道闸开闸，支持脱机运行；\n防跟车模式：支持视频防跟车、雷达/线圈防跟车两种模式，对于连续过车的场景，可实现跟车不落杆，有效解决拥堵问题；\n防护等级：机箱表面采用抗紫外线静电喷塑工艺，不起皮，不褪色，防尘防水等级符合室外设备IP54级别要求；\n电源：AC220V\n功耗：小于10W\n音质：专业回声消除和噪音抑制\n以太网：10M 100M自适应\n网络协议：TCP\n产品材质：冷轧钢板1.5mm\n屏幕供电：5V",2,"台"]
[2,"直杆变频道闸","道闸类型：直流无刷道闸；35*25*1040；\n杆件：1-6米内，直杆；\n闸杆设计：杆体采用高强度、高强轻质镁铝合金材质；\n颜色：金灰色；\n起落速度：2.5-6S可调；\n输入电源：AC220V/AC110   50/60HZ ；\n额定功率：300W   ；\n工作环境温度：-30℃～+80℃；，环境适应性强；\n闸机朝向:左/右向；\n材质：冷轧板\n遥控距离：30米  \n无线摇控功能\n电机上装有手轮装置，停电时，实现手动起落杆；\n三个按键分别控制起杆、落杆和停止；\n无触点监测：控制更精准、运行更平稳；\n具备多种接口，可接入红外线（输入低电平信号）、地感系统；",1,"台"]
[3,"直杆专用雷达","当地感线圈检测到车辆时，道闸不会下落;当红外传感器检测到车辆或行人时，道闸立即停止下落并上升:当压力电波检测到车辆或行人时，道闸也会立即停止下落并上升，有效防止车辆碰撞道闸和砸伤行人。",2,"台"]
[4,"定制控制板","定制人工开闸有记录",2,"张"]
[5,"辅料","其他安装连接设备所需的辅材由供应商根据现场安装需要自行准备",1,"批"]
[6,"车牌识别系统管理软件","车辆比对、显示进出口图片、出入场时间，车牌预录入，车辆进出数据统计、车牌识别云平台，全云端管理，支持手机管理查看现场信息",1,"套"]
[7,"加高活动板房","板房底部加高，两侧开窗（共计4个开口，含纱窗），窗户开口需略高于三轴自卸货车驾驶位（3m*6m*2.7m），完成插座及网络布线，满足用电需求，配置3p空调一套。",1,"套"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}