{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["广汉市飞虹桥"],"read":"whole","date_system":"1900"}

{"sheet":"广汉市飞虹桥","index":0,"n_rows":14,"n_cols":10,"rows_kept":14,"merged":[[0,0,0,2],[1,0,1,1],[1,4,1,8],[3,1,6,1],[7,1,10,1],[11,1,12,1]]}
[]
["附件2",{"$nulls":3},"飞虹桥传感器安全预警系统安装项目辅料采购报价清单"]
["序号","科目","服务或设备名称","型号","设备主要参数","单位","数量   ","单价（元）","总价（元）","备注"]
[1,"智能视频监控等安全设备","客流统计系统装置",null,"视场角： Horizontal 100°，Vertical 70°; 准确率： ≥98%;\n高度范围：2.2-6.0m;  覆盖范围：1.2-5.5m;   供电方式： POE（802.3af/at）/DC9~36V（标配12V）;联网方式 : 有线网络/WI-FI；功率：3.2W-7.2W；电子看板                                                                \n                                                                                                                    ","套",2,null,null,"定制（含双目摄像头、电子看板、语音播报）"]
[2,null,"电子看板立杆",null,"材质：Q235   尺寸：∅114转∅76*2000mm   表面处理：喷漆    厚度：2.0;","根",2,null,null,"定制（含电子看板、语音报警音响安装支架）"]
[3,null,"摄像头立杆",null,"材质：Q235   尺寸：∅114*3000mm+40*40*2000mm   表面处理：喷漆    厚度：3.6;","根",2,null,null,"定制（含双目摄像头2米支臂）"]
[4,null,"物联网流量卡（500M）",null,"物联网流量卡参数：流量套餐：500M/月    资费时限：1年","张",11,null,null,"1、每张卡60元/年，含5年的费用；\n2、9张卡用于9个4G姿态传感器通信；\n3、2张卡用于2台多功能数据归集器通信（采集485振动传感器和下发报警信息给现场智能音响）；"]
[5,"综合布线及安装","交流供电线缆(RVV3*1.5)",null,"国产国标","米",200]
[6,null,"网线(CAT5e)",null,"国产国标","米",100]
[7,null,"RS485通信线缆（RVS4*1.0）",null,"国产国标","米",400]
[8,null,"∅20PVC管",null,"国产国标","米",700]
[9,"综合布线及安装","安装辅料",null,null,"项",1,null,null,"不锈钢抱箍、PVC管件（三通、直接、弯头）、膨胀螺丝、胶布、扎带、管卡、安装条、雨棚等"]
[10,null,"安装人工",null,null,"项",1]
[11,"合计金额"]